

hortihenleygardening@gmail.com

07884 060239

**Quote: JPC Riverlands Ground Maintenance**

* Installation of French drain incorporating 100ml perforated land drainpipe connecting to the river Alne. Replacement of existing turf to make ground good.
* Excavation, filling of ground undulations in playground area with free draining aggregate to reduce further earth movement. Re-turfing damaged area adjacent to the play area. Removal and reinstating of rubber safety mats, where necessary, around play area.
* Provision and installation of pea gravel underneath existing seating areas.
* Safe cordoning of public areas whilst work is being undertaken.

**Quote (for works listed above): £1,275 Inclusive of provision and delivery 4 tons of pea gravel from Adams Henley FOC**

* Exploratory measures to ascertain reasons for ground movement and correction if necessary (£250 additional cost, if required).

**Quote Total: £1,525**

Please do not hesitate to get in contact if you have any queries regarding this, or future work.

Thanks

John