

hortihenleygardening@gmail.com

07884 060239

**Quote: JPC Jubilee Park**

* Provision and installation of bell-mouthed 240mm kerbed structure to North end of park to facilitate redirection of flood water, flanking the existing 5m fence and protruding an additional 5.5m.
* Compensatory measures around kerbing and gated area to provide public safety with installation of MOT base.
* Lifting existing drain grate and cleaning channel to ensure free drainage.
* Safe cordoning of public areas during works.
* Site left in a satisfactory condition.

**Quote Total: £1,700**

Please do not hesitate to get in contact if you have any queries regarding this, or future work.

Thanks

John